|  |  |  |  |
| --- | --- | --- | --- |
| **UUID** | **SERVICE** | | **CHARACTERISTIC** |
| **CLIMATE PROFILE** | | | |
| E0035607 - EC48 - 4ED0 - 9F3B - 5419C00A94FD | *Base UUID* |  | |
|  | | | |
| E0035608 - EC48 - 4ED0 - 9F3B - 5419C00A94FD | *Temperature* |  | |
| E0035609 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Current Temperature* | |
| E003560A - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Temperature Low Value (Notification Disabled)* | |
| E003560B - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Temperature High Value(Notification Disabled)* | |
| E003560C - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Temperature Alarm Set(Notification Disabled)* | |
| E003560D - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Temperature Alarm* | |
|  | | | |
| E003560E - EC48 - 4ED0 - 9F3B - 5419C00A94FD | *Light* |  | |
| E003560F - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Current Light Level* | |
| E0035610 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Light Level Low Value(Notification Disabled)* | |
| E0035611 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Light Level High Value(Notification Disabled)* | |
| E0035612 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Light Level Alarm Set(Notification Disabled)* | |
| E0035613 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Light Level Alarm* | |
|  | | | |
| E0035614 - EC48 - 4ED0 - 9F3B - 5419C00A94FD | *Humidity* |  | |
| E0035615 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Current Humidity Level* | |
| E0035616 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Humidity Low Value (Notification Disabled)* | |
| E0035617 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Humidity High Value (Notification Disabled)* | |
| E0035618 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Humidity Alarm Set (Notification Disabled)* | |
| E0035619 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Humidity Alarm* | |
|  | | | |
| E003561A - EC48 - 4ED0 - 9F3B - 5419C00A94FD | Data Logger |  | |
| E003561B - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Data Logging Enable* | |
| E003561C - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Data (When Read)* | |
| E003561D - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Read Data Enable* | |
|  | | | |
| E003561E - EC48 - 4ED0 - 9F3B - 5419C00A94FD | Device Management |  | |
| E003561F - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *DFU Mode Set (Notification Disabled)* | |
| E0035620 - EC48 - 4ED0 - 9F3B - 5419C00A94FD |  | *Switch Mode Set (Notification Disabled)* | |
| 1805 |  | *Time Stamp* | |
|  | | | |
| 180A | Device Information |  | |
| 2A29 |  | *Manufacturer Name* | |
| 2A24 |  | *Model Number* | |
| 2A23 |  | *System ID* | |
|  | | | |
| 180F | Battery Service |  | |
| 2A19 |  | *Battery Level* | |
|  |  |  | |

**UUID TABLE FOR CLIMATE PROFILE**