|  |  |  |  |
| --- | --- | --- | --- |
| **UUID** | | **SERVICE** | **CHARACTERISTIC** |
| **GROW PROFILE** | | | |
| DAF44705 – BFB0 – 4DD8 – 9293 – 62AF5F5545E31 | | *Base UUID* |  |
|  | | | |
| DAF44706 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 | *Temperature* | |  |
| DAF44707 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Current Temperature* |
| DAF44708 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Temperature Low Value (Notification Disabled)* |
| DAF44709 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Temperature High Value(Notification Disabled)* |
| DAF4470A – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Temperature Alarm Set(Notification Disabled)* |
| DAF4470B – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Temperature Alarm* |
|  | | | |
| DAF4470C – BFB0 – 4DD8 – 9293 – 62AF5F545E31 | *Light* | |  |
| DAF4470D – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Current Light Level* |
| DAF4470E – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Light Level Low Value(Notification Disabled)* |
| DAF4470F – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Light Level High Value(Notification Disabled)* |
| DAF44710 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Light Level Alarm Set(Notification Disabled)* |
| DAF44711 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Light Level Alarm* |
|  | | | |
| DAF44712 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 | *Soil Moisture* | |  |
| DAF44713 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Current Soil Moisture Level* |
| DAF44714 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Soil Moisture Level Low Value(Notification Disabled)* |
| DAF44715 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Soil Moisture Level High Value(Notification Disabled)* |
| DAF44716 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Soil Moisture Level Alarm Set(Notification Disabled)* |
| DAF44717 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Soil Moisture Level Alarm* |
|  | | | |
| DAF44718 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 | *Data Logger* | |  |
| DAF44719 – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Data Logging Enable* |
| DAF4471A – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Data (When Read)* |
| DAF4471B – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Read Data Enable* |
|  | | | |
| DAF4471C – BFB0 – 4DD8 – 9293 – 62AF5F545E31 | *Device Management* | |  |
| DAF4471D – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *DFU Mode Set (Notification Disabled)* |
| DAF4471E – BFB0 – 4DD8 – 9293 – 62AF5F545E31 |  | | *Switch Mode Set (Notification Disabled)* |
| 1805 |  | | *Time Stamp* |
|  | | | |
| 180A | *Device Information* | |  |
| 2A29 |  | | *Manufacturer Name* |
| 2A24 |  | | *Model Number* |
| 2A23 |  | | *System ID* |
|  | | | |
| 180F | Battery Service | |  |
| 2A19 |  | | *Battery Level* |

**UUID TABLE FOR GROW PROFI**