|  |  |  |  |
| --- | --- | --- | --- |
| **UUID** | **SERVICE** | | **CHARACTERISTIC** |
| **THERMO PROFILE** | | | |
| 497B8E4D - B61E - 4F82 - 8FE9 - B12CF2497338 | *Base UUID* |  | |
|  | | | |
| 497B8E4E - B61E - 4F82 - 8FE9 - B12CF2497338 | *Thermopile Temperature* |  | |
| 497B8E4F - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Current Thermopile Temperature* | |
| 497B8E50 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Thermopile Temperature Low Value (Notification Disabled)* | |
| 497B8E51 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Thermopile Temperature High Value(Notification Disabled)* | |
| 497B8E52 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Thermopile Temperature Alarm Set(Notification Disabled)* | |
| 497B8E53 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Thermopile Temperature Alarm* | |
|  | | | |
| 497B8E54 - B61E - 4F82 - 8FE9 - B12CF2497338 | *Probe Temperature* |  | |
| 497B8E55 - B61E - 4F82 - 8FE9 - B12CF2497338 |  |  | |
| 497B8E56 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Probe Temperature Low Value (Notification Disabled)* | |
| 497B8E57 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Probe Temperature High Value(Notification Disabled)* | |
| 497B8E58 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Probe Temperature Alarm Set(Notification Disabled)* | |
| 497B8E59 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Probe Temperature Alarm* | |
|  | | | |
| 497B8E5A - B61E - 4F82 - 8FE9 - B12CF2497338 | Data Logger |  | |
| 497B8E5B - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Data Logging Enable* | |
| 497B8E5C - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Data (When Read)* | |
| 497B8E5D - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Read Data Enable* | |
|  | | | |
| 497B8E5E - B61E - 4F82 - 8FE9 - B12CF2497338 | Device Management |  | |
| 497B8E5F - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *DFU Mode Set (Notification Disabled)* | |
| 497B8E60 - B61E - 4F82 - 8FE9 - B12CF2497338 |  | *Switch Mode Set (Notification Disabled)* | |
| 1805 |  | *Time Stamp* | |
|  | | | |
| 180A | Device Information |  | |
| 2A29 |  | *Manufacturer Name* | |
| 2A24 |  | *Model Number* | |
| 2A23 |  | *System ID* | |
|  | | | |
| 180F | Battery Service |  | |
| 2A19 |  | *Battery Level* | |

**UUID TABLE FOR THERMO PROFILE**